PDAC3100-D1 Windows Driver Installation and Setup


Driver Installation
1. Add Printer from control panel
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2. Don’t select “Automatically detect an install my Plug and Play printer” and Next.
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3. Next
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4. Click “Have Disk…” button
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5. Find the driver and select it.
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6. Click “OK”
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7. Next
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8. Next
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9. Click “Continue Anyway” button. Then Finish.
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Windows Driver Setup
1. start\Printers and Faxes
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2. Select printer “Properties”
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3. Select “Ports” and “Configure Port…”
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4. To Select more printing function, Please Click “Printing Preferences…”
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5. Select the printing function
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